<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="63.17" y2="0" width="0" layer="20"/>
<wire x1="63.17" y1="0" x2="63.17" y2="63.49" width="0" layer="20"/>
<wire x1="63.17" y1="63.49" x2="0" y2="63.49" width="0" layer="20"/>
<wire x1="0" y1="63.49" x2="0" y2="0" width="0" layer="20"/>
<text>Burb 
Catcher</text>
<text>Input Board</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>+</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>-</text>
<text>Stack</text>
</plain>
<libraries>
<library name="74xx-us">
<description>&lt;b&gt;TTL Devices, 74xx Series with US Symbols&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Texas Instruments &lt;i&gt;TTL Data Book&lt;/i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;Volume 1, 1996.
&lt;li&gt;TTL Data Book, Volume 2 , 1993
&lt;li&gt;National Seminconductor Databook 1990, ALS/LS Logic
&lt;li&gt;ttl 74er digital data dictionary, ECA Electronic + Acustic GmbH, ISBN 3-88109-032-0
&lt;li&gt;http://icmaster.com/ViewCompare.asp
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO16">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="1X2-3.5MM">
</package>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X13">
<description>&lt;h3&gt;Plated Through Hole -13 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:13&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_13&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="IC1" library="74xx-us" package="SO16" value="74LS251D">
<attribute name="MF" value=""/>
<attribute name="MPN" value="74HC151D"/>
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="26M7760"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="adafruit" package="1X2-3.5MM" value="1X2-3.5MM">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="39357-0002"/>
<attribute name="OC_NEWARK" value="72K2104"/>
</element>
<element name="J10" library="SparkFun-Connectors" package="1X13" value="Male (Top)">
<attribute name="MF" value=""/>
<attribute name="MPN" value="LS-00004"/>
<attribute name="OC_NEWARK" value="75X1508"/>
</element>
<element name="J2" library="adafruit" package="1X2-3.5MM" value="1X2-3.5MM">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="39357-0002"/>
<attribute name="OC_NEWARK" value="72K2104"/>
</element>
<element name="J3" library="adafruit" package="1X2-3.5MM" value="1X2-3.5MM">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="39357-0002"/>
<attribute name="OC_NEWARK" value="72K2104"/>
</element>
<element name="J4" library="adafruit" package="1X2-3.5MM" value="1X2-3.5MM">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="39357-0002"/>
<attribute name="OC_NEWARK" value="72K2104"/>
</element>
<element name="J5" library="adafruit" package="1X2-3.5MM" value="1X2-3.5MM">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="39357-0002"/>
<attribute name="OC_NEWARK" value="72K2104"/>
</element>
<element name="J6" library="adafruit" package="1X2-3.5MM" value="1X2-3.5MM">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="39357-0002"/>
<attribute name="OC_NEWARK" value="72K2104"/>
</element>
<element name="J7" library="adafruit" package="1X2-3.5MM" value="1X2-3.5MM">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="39357-0002"/>
<attribute name="OC_NEWARK" value="72K2104"/>
</element>
<element name="J8" library="adafruit" package="1X2-3.5MM" value="1X2-3.5MM">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="39357-0002"/>
<attribute name="OC_NEWARK" value="72K2104"/>
</element>
<element name="J9" library="SparkFun-Connectors" package="1X13" value="Female(Bottom)">
<attribute name="MF" value=""/>
<attribute name="MPN" value="LS-00006"/>
<attribute name="OC_NEWARK" value="75X1513"/>
</element>
<element name="LED1" library="adafruit" package="CHIP-LED0805" value="Red">
<attribute name="MF" value=""/>
<attribute name="MPN" value="KPTD-2012LVSURCK"/>
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="50AC9311"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="adafruit" package="CHIP-LED0805" value="Blue">
<attribute name="MF" value=""/>
<attribute name="MPN" value="KPTD-2012LVQBC-D"/>
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="50AC9310"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="adafruit" package="CHIP-LED0805" value="Red">
<attribute name="MF" value=""/>
<attribute name="MPN" value="KPTD-2012LVSURCK"/>
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="50AC9311"/>
<attribute name="VALUE"/>
</element>
<element name="LED4" library="adafruit" package="CHIP-LED0805" value="Blue">
<attribute name="MF" value=""/>
<attribute name="MPN" value="KPTD-2012LVQBC-D"/>
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="50AC9310"/>
<attribute name="VALUE"/>
</element>
<element name="LED5" library="adafruit" package="CHIP-LED0805" value="Red">
<attribute name="MF" value=""/>
<attribute name="MPN" value="KPTD-2012LVSURCK"/>
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="50AC9311"/>
<attribute name="VALUE"/>
</element>
<element name="LED6" library="adafruit" package="CHIP-LED0805" value="Blue">
<attribute name="MF" value=""/>
<attribute name="MPN" value="KPTD-2012LVQBC-D"/>
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="50AC9310"/>
<attribute name="VALUE"/>
</element>
<element name="LED7" library="adafruit" package="CHIP-LED0805" value="Red">
<attribute name="MF" value=""/>
<attribute name="MPN" value="KPTD-2012LVSURCK"/>
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="50AC9311"/>
<attribute name="VALUE"/>
</element>
<element name="LED8" library="adafruit" package="CHIP-LED0805" value="Blue">
<attribute name="MF" value=""/>
<attribute name="MPN" value="KPTD-2012LVQBC-D"/>
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="50AC9310"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="R0805" value="10k">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ERJ-U02F1002X"/>
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="51W2917"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="R0805" value="10k">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ERJ-U02F1002X"/>
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="51W2917"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="R0805" value="10k">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ERJ-U02F1002X"/>
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="51W2917"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="adafruit" package="R0805" value="10k">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ERJ-U02F1002X"/>
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="51W2917"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="adafruit" package="R0805" value="10k">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ERJ-U02F1002X"/>
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="51W2917"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="adafruit" package="R0805" value="10k">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ERJ-U02F1002X"/>
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="51W2917"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="adafruit" package="R0805" value="10k">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ERJ-U02F1002X"/>
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="51W2917"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="adafruit" package="R0805" value="10k">
<attribute name="MF" value=""/>
<attribute name="MPN" value="ERJ-U02F1002X"/>
<attribute name="NAME"/>
<attribute name="OC_NEWARK" value="51W2917"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="8"/>
<contactref element="J6" pad="1"/>
<contactref element="IC1" pad="7"/>
<contactref element="J10" pad="2"/>
<contactref element="J9" pad="12"/>
<contactref element="J8" pad="1"/>
<contactref element="J7" pad="1"/>
<contactref element="J5" pad="1"/>
<contactref element="J4" pad="1"/>
<contactref element="J3" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="16"/>
<contactref element="R8" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$176">
<contactref element="IC1" pad="9"/>
<contactref element="J9" pad="11"/>
<contactref element="J10" pad="3"/>
</signal>
<signal name="N$207">
<contactref element="IC1" pad="10"/>
<contactref element="J9" pad="10"/>
<contactref element="J10" pad="4"/>
</signal>
<signal name="N$16">
<contactref element="IC1" pad="11"/>
<contactref element="J9" pad="9"/>
<contactref element="J10" pad="5"/>
</signal>
<signal name="+5V">
<contactref element="J9" pad="13"/>
<contactref element="J10" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="J1" pad="2"/>
<contactref element="IC1" pad="4"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="N$2">
<contactref element="J2" pad="2"/>
<contactref element="IC1" pad="3"/>
<contactref element="LED2" pad="C"/>
</signal>
<signal name="N$3">
<contactref element="J3" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="LED3" pad="C"/>
</signal>
<signal name="N$5">
<contactref element="J4" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="LED4" pad="C"/>
</signal>
<signal name="N$6">
<contactref element="J5" pad="2"/>
<contactref element="IC1" pad="15"/>
<contactref element="LED5" pad="C"/>
</signal>
<signal name="N$7">
<contactref element="J6" pad="2"/>
<contactref element="IC1" pad="14"/>
<contactref element="LED6" pad="C"/>
</signal>
<signal name="N$8">
<contactref element="J7" pad="2"/>
<contactref element="IC1" pad="13"/>
<contactref element="LED7" pad="C"/>
</signal>
<signal name="N$9">
<contactref element="J8" pad="2"/>
<contactref element="IC1" pad="12"/>
<contactref element="LED8" pad="C"/>
</signal>
<signal name="N$10">
<contactref element="R8" pad="2"/>
<contactref element="LED8" pad="A"/>
</signal>
<signal name="N$11">
<contactref element="R7" pad="2"/>
<contactref element="LED7" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$12">
<contactref element="R2" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$13">
<contactref element="R3" pad="2"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$23">
<contactref element="R4" pad="2"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="N$24">
<contactref element="R5" pad="2"/>
<contactref element="LED5" pad="A"/>
</signal>
<signal name="N$25">
<contactref element="R6" pad="2"/>
<contactref element="LED6" pad="A"/>
</signal>
<signal name="N$14">
<contactref element="IC1" pad="5"/>
<contactref element="J9" pad="8"/>
</signal>
<signal name="N$15">
<contactref element="J9" pad="7"/>
<contactref element="J10" pad="6"/>
</signal>
<signal name="N$17">
<contactref element="J9" pad="6"/>
<contactref element="J10" pad="7"/>
</signal>
<signal name="N$18">
<contactref element="J9" pad="5"/>
<contactref element="J10" pad="8"/>
</signal>
<signal name="N$19">
<contactref element="J9" pad="4"/>
<contactref element="J10" pad="9"/>
</signal>
<signal name="N$20">
<contactref element="J9" pad="3"/>
<contactref element="J10" pad="10"/>
</signal>
<signal name="N$21">
<contactref element="J9" pad="2"/>
<contactref element="J10" pad="11"/>
</signal>
<signal name="N$22">
<contactref element="J9" pad="1"/>
<contactref element="J10" pad="12"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
